Пример вызова прерывания

section .data hello: db 'Hello world!',10 ; 'Hello world!' plus a linefeed character helloLen: equ $-hello ; Length of the 'Hello world!' string ; (I'll explain soon) section .text global _start _start: mov eax,4 ; The system call for write (sys_write) mov ebx,1 ; File descriptor 1 - standard output mov ecx,hello ; Put the offset of hello in ecx mov edx,helloLen ; helloLen is a constant, so we don't need to say ; mov edx,[helloLen] to get it's actual value int 80h ; Call the kernel mov eax,1 ; The system call for exit (sys_exit) mov ebx,0 ; Exit with return code of 0 (no error) int 80h

Задание. Напишите процедуру вывода на экран содержимого регистра rax в 16ричном формате (это более простой случай, 10ричный формат гораздо сложнее).